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2011-2014 F150 EcoBoost Tuning Device
Installing Stock or Custom Calibration Files
Plug the Device into the OBD-II port with the engine off. Ensure the cable is securely connected and does not become disconnected during the session. Put the vehicle in accessory mode by turning the key forward and DO NOT turn off the key until the transfer is complete; follow the prompts on the display. After flashing back to stock, disconnect the battery for 10 minutes.
Before Programming:

1) Turn everything off (A/C, radio, auto lights, etc.)
2) Get in the vehicle and shut the doors

3) Set the device on a stable flat surface

4) Don’t touch anything until it finishes
5) Don't let anyone else approach the car and open the doors, turn on the radio, etc.
Engineering Mode:

Holding the N and Up buttons simultaneously while plugging the device into the OBD-II port will enter engineering mode. Once in engineering mode, you can see voltage and the ECU CAL/Strategy and SW ID, which can be found in the same menu as the strategy. If you take your vehicle to the dealer for service, you may want to verify the strategy code to make sure the tune you are installing is the same strategy currently in your vehicle.
NOTE: DO NOT TOW WITH A PERFORMANCE TUNE. It could cause damage to the engine, turbos, or catalytic converters.  ALWAYS USE A TOW SPECIFIC TUNE when towing.
