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2017+ GM Tuning Device
Plug the Device into the OBD-II port with the engine off. Ensure the cable is securely connected and does not become disconnected during the session. Put the vehicle in accessory mode by turning the key forward and DO NOT turn off the key until the transfer is complete.  On vehicles with a push button ignition put the vehicle into accessory mode by holding the start button for 10-12 seconds without applying the brake. The start button should now have a green light.   
Step 1 – Connect the Mycal tuning device to your vehicle’s diagnostic port below driver side dash.  This should result in an "Update Required" message just after reading/clearing DTCs.  Must clear these codes if any.
Step 2 - Install the Tuner Update Software from the links provided below on to a Windows PC. Use the update application to update your tuner, and please enter your email to be notified when the update is ready when prompted during this 1st update.  This may take up to 2 business days, but we'll get to this ASAP.
Step 3 - Use Tuner Update Software to update the tuner after being notified that the update is available by email.
 
Step 4 - Connect Loader to vehicle and follow the on screen prompts to enter programmer mode to let it read and copy your factory tune files.   You will see a percentage displayed during the read which must reach 100%.

Step 5- Once completed please email your full name, year make model, VIN of the vehicle, mods (if any), fuel octane, & device serial # to tuning@livernoismotorsports.com and await further instructions.

Please follow the instructions below to install the tuner update application. Once installed open the new program labeled Tuner update application, connect the tuner to the PC with the supplied USB cable, and select "Update" to complete the file transfer.
https://www.livernoismotorsports.com/DOWNLOADS
[bookmark: _GoBack] Note the location on the PC as to where the setup file is being saved.. Go to the location on the PC where the files were downloaded to. Double-click (run) file setup_web.exe  This will start the installer that installs the Tuner Update Software.  Follow the on screen prompts as usual to install\update the application. After step 5 is complete be sure to open the tuner update application you have just installed, plug in the tuner if not already connected, and select update tuner to send your vehicles information to our server. Feel free to give us a call if you have any questions (313)561-5500.
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