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                                     Chevrolet SS / Pontiac G8 Tuning Device

Plug the Device into the OBD-II port with the engine off. Ensure the cable is securely connected and does not become disconnected during the session. Put the vehicle in accessory mode by holding the start button for 10-12 seconds without applying the brake. The start button should now have a green light.   Follow the prompts on the display to enter programing mode.   The device will then read out the vehicle’s factory calibration.  When the reading process has finished getting the data from the vehicle you will see a message that there are no tunes on the device and be prompted to disconnect from the vehicle.   
 Once completed please install the tuner update application on to your PC and select update tuner to send us your vehicles information.  Once the device has been updated please email your full name, the VIN number of the vehicle, mods (if any), fuel octane, & device serial # to tuning@livernoismotorsports.com


Please follow the instructions below to install the tuner update application. Once installed open the new program labeled Tuner update application V2, connect the tuner to the PC with the supplied USB cable, and select "Update tuner" to complete the file transfer.

Download the setup file below if your Anti Virus or firewall does not attempt to quarantine it.  If you have any issues with the Antivirus or firewalls please adjust as needed or temporarily disable them.
http://www.webservice99.com/downloads/tunerupdateapplication/V2/Current/setup_web.exe

[bookmark: _GoBack]Once the installation of the application is complete be sure to open the tuner update application you have just installed, plug in the tuner if not already connected, and select update tuner to send your vehicles information to our server. Feel free to give us a call if you have any questions (313)561-5500.
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