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LIVERNOIS MOTORSPORTS CHRYSLER & DODGE TUNING DEVICE
*Please ensure the vehicle has a fully charged battery before connecting the tuning device.*

[bookmark: _GoBack]Plug the Device into the OBD-II port with the engine off. Ensure the cable is securely connected and does not become disconnected during the session. Put the vehicle in run mode by turning the key all the way forward but do not start.  Keyless vehicles you will need to press the ignition start button to put it in RUN mode, but do not start the vehicle.  Follow the prompts on the display to enter tuning / programming mode and select the option to install custom tuning.  The device will get to a point where it tells you there are no tune files loaded on the device yet which is normal.  This will allow the device to read a copy of your factory calibration codes which we need to create your custom tune.
Once completed please install the tuner update application on to your PC and select update tuner to send us your vehicles factory information.  Once the device has been updated please email your full name, year, make, model, engine size, and VIN of the vehicle, along with any modifications done to the vehicle, fuel octane being used, & your tuning device’s serial # to tuning@livernoismotorsports.com

Please follow the instructions below to install the tuner update application.  Once installed open the new program labeled Tuner update application V2, connect the tuner to the PC with the supplied USB cable, And select "Update tuner" to complete the file transfer.
Single file installer 
http://www.webservice99.com/downloads/tunerupdateapplication/V2/Current/setup_web.exe

image1.png




